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	                   Annex F1/2 to the Certificate No. 1441
SCOPE of ACCREDITATION

of the

Testing Laboratory
GEODYNAMIKI TEHNIKI I.K.E
 


	Materials/ Products to be tested
	Types of test/ Properties to be  measured
	Applied Standards/ Techniques to be used

	Physical and Chemical testing

	Aggregates/Soils
	1. Tests for geometrical properties of aggregates -                                                         Part 1: Determination of particle size distribution - Sieving method
	EΛOT EN 933-1:2012

	
	2. Tests for geometrical properties of aggregates -                                                         Part 8: Assessment of fines - Sand equivalent test
	EΛOT EN 933-8:2012 +A1:2015

	
	3. Standard Test Method for Density and Unit Weight of Soil in Place by Sand-Cone Method
	ΥΠΕΧΩΔΕ/ΚΕΔΕ Ε106-86/2

	
	4. Standard Test Methods for In-Place Density and Water Content of Soil and Soil-Aggregate by Nuclear Methods
	ASTM D6938-23

	Bituminous Mixtures
	1. Bituminous mixtures - Test methods -           Part 1:  Soluble binder content
	EΛOT ΕΝ 12697-1:2020

	
	2. Bituminous mixtures - Test methods -          Part 2: Determination of particle size distribution
	EΛOT ΕΝ 12697-2:2025


	
	3. Bituminous mixtures - Test methods -          Part 5: Determination of the maximum density
	EΛOT ΕΝ 12697-5:2018

	
	4. Bituminous mixtures - Test methods -         Part 6: Determination of bulk density of bituminous specimens
	EΛOT ΕΝ 12697-6:2020



	
	5.       Bituminous mixtures - Test methods - 

Part 8: Determination of void characteristics of bituminous specimens 
	EΛOT ΕΝ 12697-8:2018

	
	6.        Bituminous mixtures. Test methods - 
Part 29: Determination of the dimensions of a bituminous specimen
	EΛOT ΕΝ 12697-29:2020



	Mechanical Testing

	Aggregates
	1.    Tests for mechanical and physical properties of aggregates -                                                            Part 2: Methods for the determination of resistance to fragmentation (Los Angeles test)
	EΛOT EN 1097-2:2020

	Bituminous Mixtures 
	1.        Bituminous mixtures - Test methods -                Part 30: Specimen preparation by impact compactor                                 
	EΛOT ΕΝ 12697-30:2019

	
	2.        Bituminous mixtures - Test methods -            Part 34: Marshall test
	EΛOT ΕΝ 12697-34:2020




Site of assessment: Laboratory permanent premises, 8 Amfitritis str, Pylaia, Thessaloniki, Greece.
Approved signatory: Tsolakis Ioannis.
This Scope of Accreditation replaces the previous one dated 10.01.2025
The Accreditation Certificate No. 1441, to ELOT EN ISO/IEC 17025:2017, is valid until  09.01.2030.
     Athens, 08.01.2026
      Konstantinou Evangelos Apostolos

CEO of ESYD
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