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	Annex F1/5 to the Certificate No. 1200-2

SCOPE of ACCREDITATION
of the 
Testing Laboratory 
of
‘‘G. KARYDIS - DOMO+LYSISLAB – 
Laboratory of Structural Assessment and Protection’’



	[bookmark: _Hlk30506016][bookmark: _Hlk21798166]
Tested Materials / Products
	
Types of Test / Properties to be measured / Procedures

	
Applied Standards / 
Techniques to be used

	
	Non-Destructive Testing
	

	Hardened Concrete
	1. Determination of rebound number in concrete structures. 
	EN 12504 - 2: 2021

	
	2. Determination of ultrasonic pulse velocity in concrete structures. 
	EN 12504 - 4: 2021

	Metals / 
Hardened Concrete
	3. Investigation of steel reinforcement concrete members with the operation of electromagnetic device. Estimation the position, depth and size of steel reinforcement rods. 
	BS 1881 - 204: 1988

	
	4. Standard test method for corrosion potentials of uncoated reinforcing steel in concrete.
	ASTM C 876 – 22B

	Coatings – Lining Systems
	5. Determination of the film thickness of coatings on metallic and non-metallic substrate using an ultrasonic gage. 
	EN ISO 19397: 2024



	
Tested Materials / Products
	
Types of Test / Properties to be measured / Procedures

	
Applied Standards / 
Techniques to be used

	
	Physical Testing
	

	Concrete
	1. Determination of carbonation depth in hardened concrete by the phenolphthalein method.
	EN 14630: 2007

	
	2. Making and curing specimens for strength tests.
	EN 12390 - 2: 2019

	Coatings – Lining Systems
	3. Determination of dry film thickness by wedge-cut method.
	EN ISO 19399: 2016
Method Α - (Scribe)

	Mechanical Testing

	Hardened Concrete
	1. Determination of concrete strength at cored specimens of hardened concrete. Taking, examining and testing in compression. 
	EN 12504-1:2019

	
	2. Determination of compressive strength of hardened concrete. 
	EN 12390-3:2019
Hellenic Concrete Technology Regulation (KTS) 2016

	Cementitious Mortars / Cementitious Slurries 
	3. Determination of adhesion strength (Pull-Off) for products and systems used for repair and protection of reinforced concrete structures.
	EN 1542: 1999
Testing only on site. 
Does not comply with §2 §4.1, 4.2, 4.3, 4.4, 4.12, §5, §6.

	Fiber Reinforced Polymers (FRP) Laminates
	4. Determination of adhesion strength (Pull-Off) for FRP laminate systems bonded to concrete and masonry substrates.
	ASTM D7522 / D7522M - 21

	
Coatings – Lining Systems
	5. Determination of adhesion strength (Pull-Off) for paints and varnishes.
	EN ISO 4624: 2023
Method Β
(Rigid substrates)
Testing only on site. 
Does not comply with §6, §7, §8.1, 8.2



Site of assessment: Laboratory permanent premises: Distomou 97 - Kolonos - Athens - 10443, Athens 
Approved signatories: Georgios Karydis, Besian (Ioannis) Tsaousdelo

This Scope of Accreditation replaces the previous one dated July 25th, 2024
The Accreditation Certificate No. 12007 to ELOT EN ISO/IEC 17025:2017, is valid until August 9th, 2029. 

Athens, March 21st, 2025


                    					 Konstantinou Evangelos Apostolos
CEO of ESYD
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